Eastwood TIG Welder Safety Tips

1. Before beginning, be sure the work surface is cleaned of any oils, coatings or other materials, which can ignite and/or emit dangerous fumes or vapors.
2. The work area and the equipment must be dry. Avoid welding in high humidity and with excessive perspiration.
3. Keep all cords as far away from the welder unit as possible to avoid any possibility of arcing to the internal transformer. This includes the power cord, torch feed cord and ground clamp cord.
4. Remove all metallic objects from clothing. Position yourself over a rubber at while welding and use a non-metallic chair.
5. Never bypass the ground plug. Grounding is necessary for proper operation of the unit and reduces shock hazard.
6. Use heavy duty welding gloves (#12590) and an auto darkening welding mask (#12099)

For more information see <http://www.eastwood.com/eastwood-s-ac-dc-tig-200-welder.html> or contact Connie LaMotta, 845.596.6091 or conniela@mac.com