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CPM® Powder Metal Tool Steel Combined with Diehl Steel’s Accu-Square™ Process is Perfect for the Most Demanding Applications
CINCINNATI, OH (June 23, 2014) – Diehl Steel stocks and sells a wide variety of grades of CPM® powder metal products designed for customer’s most demanding applications. The CPM® process eliminates alloy segregation and produces more highly alloyed grades of steel which cannot be produced by conventional steelmaking.  The process results in a very fine, more uniform carbide distribution and imparts improved toughness and grindability, superior dimensional stability, as well as outstanding hardness, wear resistance and heat resistance compared to conventional tool steel products.  

When combined with Diehl’s Accu-Square process the result is powder metal pre-squared on all six sides to the toolmaker’s requested tolerance range.  This reduces or eliminates the need for further squaring of the blocks, and is designed to save time and cut costs.
Diehl Steel offers a range of grades to accommodate most applications where powder metal tool steel is required.  

· CPM® REX M-4, a powder metal tool steel that offers improved cutting tool life compared to conventionally wrought M-1, M-2, M-7 and other lower-alloyed high speed steels. 
· CPM® REX 76, a super high speed steel that contains high carbon, vanadium and cobalt for abrasion resistance comparable to T15 and superior red hardness. 
· CPM® REX T15, a tungsten type super high speed steel containing high vanadium for excellent abrasion resistance, and cobalt for good red hardness. 
· CPM® REX 45, an 8% cobalt super high speed steel which has excellent hot hardness along with good wear resistance and toughness.


- More - 

· CPM® 1V®, a medium-carbon, powder metal tool steel that exhibits very high impact toughness.

· CPM® 3V®, an air-hardening, powder metal tool steel with a unique chemical composition that results in tooling with an outstanding combination of high impact toughness and wear resistance. 
· CPM® 9V®, a powder metal tool steel that provides very high wear resistance in combination with impact toughness. 
· CPM® 10V®, a versatile air hardening, powder metal tool and die steel which provides extremely high wear resistance and  relatively high impact toughness. 
· CPM® 15V®, a powder metal tool steel that has exceptional wear resistance. It provides more wear resistance and longer tool life in applications similar to CPM® 10V®.
About Diehl Steel
Diehl Steel is an international supplier of quality tool steel, alloy steel, CPM® powder metal, mold steel, carbon steel, stainless steel and aluminum products and services.   The company offers standard and custom cut and machined sizes of flats, bars, squares, sheets, plates, drill rod, hollowbar and rounds.  With its unique Accu-Square process, the company can square metal block to toolmaker tolerances.  Diehl Steel focuses on serving the rapid turn-around needs of the tool and die, mold shop, machine shop, and O.E.M. industries, typically shipping in-stock items in 24 to 48 hours.
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